[image: ]



Sequence of Events
	[bookmark: _Hlk234920121]Stage:
	Responsible parties:

	Identification of project that will increase existing electrical demand at given school site.

Engage professional services to complete Specialised Report. 

	· Project manager.
· Design manager.
· Delivery manager.



	Conduct review of existing school electrical infrastructure in relation to planned electrical installation. 
Conduct necessary site visits.
Prepare and provide Specialised Report.

Submit Specialised Report to The New Zealand School Property Agency electrical.services@schoolproperty.govt.nz for review, endorsement and guidance.
	· Certified electrical engineer; or
· Licensed electrician; or
· A competent person with a similar level of expertise.


	Scenario 1:
If determined that existing electrical infrastructure will accommodate additional electrical demand (with or without deployment of additional technologies):

Proceed with a Certified Electrical Design for planned electrical installation.
	· Project manager.
· Design manager.
· Delivery manager.
· Certified electrical engineer; or
· Licensed electrician; or
· A competent person with similar level of expertise.

	Scenario 2:
If determined that existing electrical infrastructure will NOT accommodate additional electrical demand (despite potential deployment of additional technologies):
Engage professional services to complete an Electrical Infrastructure Capacity Report Information can be found at Designing Quality Learning Spaces.

Submit Electrical Infrastructure Capacity Report to The New Zealand School Property Agency electrical.services@schoolproperty.govt.nz for review, endorsement and guidance.
	· Certified electrical engineer; or
· Licensed electrician; or
· A competent person with similar level of expertise.
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